Class Index | File Index

## Classes

- _global_
- AccessController
- APDU
- AuthenticationObject
- CAConnection
- ChipAuthentication
- ChipAuthenticationDomainParameterInfo
- ChipAuthenticationInfo
- ChipAuthenticationPublicKeyInfo
- CommandInterpreter
- CRLGenerator
- CVC
- CVCCA
- CVCertificateStore
- DataUnitAPDU
- DF
- DKEK
- DNEncoder
- EAC20
- EAC2CVCertificateGenerator
- EAC2CVRequestGenerator
- FCP
- File
- FileSelector
- FileSystemIdObject
- FSNode
- GPSCP03
- HSMCVCertificateStore
- HSMKeyStore
- LinearEF
- ManagePKA
- P11CVCertificateStore
- PACE
- PACEDomainParameterInfo
- PACEInfo
- PaperKeyEncoding
- PKCS10Generator
- PublicKeyReference
- RAMClient
- RestrictedIdentificationDomainParameterInfo
- RestrictedIdentificationInfo
- SecureChannelHandler
- SecureMessagingCommandAPDUDecoder
- SecurityEnvironment
- SignatureKey
- SmartCardHSM
- SmartCardHSMCrypto
- SmartCardHSMInitializer
- SmartCardHSMKey
- SmartCardHSMKeySpecGenerator
- SmartCardHSMSymmetricKeySpecGenerator
- TransparentEF
- TrustAnchor
- X509CertificateGenerator
- X509CertificateIssuer
- X509CertificateStore
- X509Signer

# Class SmartCardHSM

Class implementing support for SmartCard-HSM access
Defined in: SmartCardHSM.js.

Class Summary
Constructor Attributes | Constructor Name and Description
--- | ---
| SmartCardHSM(card) Create a SmartCard-HSM access object

Method Summary
Method Attributes | Method Name and Description
--- | ---
| addCACertificateToMap(cert, id, label) Add a new CA certificate to the map
| addKeyToMap(key) Add a new key to the map of keys
| associateXKEKKeyDomain(keyDomain, keyDomainUID, keyDomainAssociation, keyDomainAssociation) Associate XKEK Key Domain
<static> | SmartCardHSM.buildCertDescription(commonObjectFlags, label, pubKey, certFID) Create a PKCS#15 certificate description
<static> | SmartCardHSM.buildDataObjectDescription(label, commonObjectFlags, fid, applicationName) Create a PKCS#15 data object description
<static> | SmartCardHSM.buildGAKPwithECC(innerCAR, algo, chr, dp, outerCAR, privateKey) Build input for Generate Asymmetric Key Pair command for generating an ECC key pair
<static> | SmartCardHSM.buildGAKPwithRSA(innerCAR, algo, chr, keysize, outerCAR) Build input for Generate Asymmetric Key Pair command for generating a RSA key pair
<static> | SmartCardHSM.buildKeyDomainDescription(label) Create a PKCS#15 like KeyDomain description
<static> | SmartCardHSM.buildPrkDforECC(keyid, label, keysize) Create a PKCS#15 PrivateECCKey description
<static> | SmartCardHSM.buildPrkDforRSA(keyid, label, modulussize) Create a PKCS#15 PrivateRSAKey description
<static> | SmartCardHSM.buildSKDforAES(keyid, label, keysize) Create a PKCS#15 SecretKey description
| changeInitializationCode(initializationCode, newInitializationCode) Change InitializationCode
| changeUserPIN(currentPIN, newPIN) Change User PIN
| createXKEKKeyDomain(keyDomain, keyDomainMembership, keyDomainMembership) Create XKEK Key Domain
| decipher(keyid, algo, data) Decipher cryptogram or agree shared secret using Diffie-Hellman
<static> | SmartCardHSM.decodeAlgorithmList(list) Decode algorithm list and return string array with names
| deleteDataObject(label) Delete the data object references by the label.
| deleteFile(fid) Delete file system object (EF or key)
| deleteKEK(keyDomain) Delete the key encryption key in a key domain
| deleteKeyDomain(keyDomain) Delete the empty key domain
| deriveSymmetricKey(id, algo, derivationParam) Derive Symmetric Key
| deriveXKEK(keyDomain, derivationParam, derivationParam) Derive XKEK
| determineFreeCAId() Determine an unused CA certificate identifier
<static> | SmartCardHSM.determineFreeFid(the, the) Determine a free FID in the list of FID for the given prefix.
<static> | SmartCardHSM.determineFreeId(the, the) Determine a free id in the list of FID for the given prefix.
| determineFreeKeyId() Determine an unused key identifier
<static> | SmartCardHSM.disableUTSRCA() Remove Root Certificate of Development SRCA Always call this on a productive system
<static> | SmartCardHSM.dumpKeyData(keydata) Dump C-Data of Generate Asymmetric Key Pair command
<static> | SmartCardHSM.encodeAlgorithmList(list) Parse and encode the algorithm list containing either algorithm ids or names
| enumerateCACertificates() Enumerate CA certificates
| enumerateDataObjects() Enumerate Data Objects
| enumerateKeys() Enumerate key objects in the SmartCard-HSM and build the map of keys
| enumerateObjects() Enumerate Objects
| generateAsymmetricKeyPair(newkid, signkid, keydata) Generate an asymmetric key pair
| generateRandom(length) Generate random data
| generateSymmetricKey(newkid, algo, keydata) Generate a symmetric key
| getCACertificate(label) Return CA certificate with label
| getCrypto() Get crypto object
| getDataObjectFileIdentifier(label) Return the file identifier containing the data object.
| getFreeMemory() Determine free memory
| getKey(labelOrId) Get a key reference object
| getKeyDomainLabel(keyDomain) Return the label associated with the key domain or undefined.
| getKeyIds() Get key ids
| getKeys() Return a list of key objects
| getLabel() Get Token Label
| getNativeCardService() Return the native OCF SmartCardHSMCardService
| getProvisioningURL() Get ProvisioningURL
| getTokenManagementKeyKCV() Get Key Check Value of Token Management Key
| getTokenManagementKeySalt() Get salt for SO-PIN derivation using the Token Management Key
| getVersionInfo() Return a string describing the SmartCard-HSM Version
| hasDataObject(label) Check if the data object is present
| hasFile(fid) Try selecting the file to see if is present
| importDataObject(label, privObj, data) Import a data object
| importEncryptedKeyShare(keyshare, password, keyDomain) Decrypt and import a DKEK share
| importKeyShare(keyDomain, keyshare) Import DKEK share or query status
| initDevice(options, initialPIN, initializationCode, retryCounterInitial, keyshares) Initialize device and clear all keys and files
| isInitialized() Return true is SmartCard-HSM is initialized
| isPINResetEnabled() Check if the RESET RETRY COUNTER command can reset the PIN
| isResetRetryCounterEnabled() Check if the RESET RETRY COUNTER command is enabled
| logout() Logout
| openSecureChannel(crypto, devAuthPK) Open a secure channel using device authentication
<static> | SmartCardHSM.parseCertificateList(a) Parse list of CVC in a binary blob
| parseKeyDomainStatus(status) Parse the key domain status returned from the device
| queryInitializationCodeStatus() Request Initialization Code Status
| queryKeyDomainStatus(keyDomain) Query the status of the key domain
| queryPINStatus(p2) Request PIN Status Information
| queryUserPINStatus() Request PIN Status Information
| readBinary(fid, offset, length) Read transparent EF referenced by file identifier
| selectFile(fid) Select the file or key an return the FCP
<static> | SmartCardHSM.setTrustedSRCACertificates(srcalist) Set the list of trusted SRCA certificates
| sign(keyid, algo, data) Sign data using referenced key
<static> | SmartCardHSM.stripLeadingZeros(value) Strips leading zeros of a ByteString
| unblockUserPIN(initializationCode, newPIN) Unblock and set User PIN
| unwrapAndReplaceKey(id, keyblob) Replace symmetric key value encrypted under current key
| unwrapKey(id, keyblob) Unwrap key with DKEK
| updateBinary(fid, offset, data) Update transparent EF referenced by file identifier
| updateKey(key) Update key attributes, in particular the use counter
| validateCertificateChain(crypto) Validate device certificate chain
<static> | SmartCardHSM.validateCertificateChain(crypto, devAutCert) Validate device certificate chain
| verifyCertificate(cvc) Verify card verifiable certificate
| verifyUserPIN(userPIN) Verify User PIN
| wrapKey(id) Wrap key under DKEK

Class Detail
SmartCardHSM(card)
Create a SmartCard-HSM access object

Parameters:
{Card} card
  the card object

Method Detail
addCACertificateToMap(cert, id, label)
Add a new CA certificate to the map

Parameters:
{X509} cert
  the CA certificate
{Number} id
  the corresponding id
{String} label
  the corresponding label

addKeyToMap(key)
Add a new key to the map of keys

Parameters:
{HSMKey} key
  the HSM key

{Object} associateXKEKKeyDomain(keyDomain, keyDomainUID, keyDomainAssociation, keyDomainAssociation)
Associate XKEK Key Domain

Parameters:
{Number} keyDomain
  number of key domain in the range 0 to the maximum defined in the INITIALIZE DEVICE command
{ByteString} keyDomainUID
  a encoded TLV object with tag 51 containing the key domain uid of the associated domain
{ByteString} keyDomainAssociation
  a encoded TLV object with tag 56 or 57
keyDomainAssociation

Returns:
  object with properties sw{Number}, shares{Number}, outstanding{Number}, kcv{ByteString} and the key domain UID{ByteString}

<static> {ASN1} SmartCardHSM.buildCertDescription(commonObjectFlags, label, pubKey, certFID)
Create a PKCS#15 certificate description

Parameters:
{ByteString} commonObjectFlags
  default value is '0640'
{String} label
  the key label
{Key} pubKey
  the public key
{ByteString} certFID
  the file identifier of the certificate

Returns:
  the certificate description

<static> {ASN1} SmartCardHSM.buildDataObjectDescription(label, commonObjectFlags, fid, applicationName)
Create a PKCS#15 data object description

Parameters:
{String} label
  the key label
{ByteString} commonObjectFlags
  default value is '0640'
{ByteString} fid
  the file identifier of the data object
{String} applicationName
  the application name (Default "SmartCard-HSM")

Returns:
  the Data Object Description

<static> {ByteString} SmartCardHSM.buildGAKPwithECC(innerCAR, algo, chr, dp, outerCAR, privateKey)
Build input for Generate Asymmetric Key Pair command for generating an ECC key pair

Parameters:
{PublicKeyReference} innerCAR
  the CA the request shall be directed to
{ByteString} algo
  the public key algorithm
{PublicKeyReference} chr
  the certificate holder reference associated with this key
{Key} dp
  the domain parameter for the key
{PublicKeyReference} outerCAR
  the certificate holder reference of the public key for verifying the outer signature
{Key} privateKey
  optional parameter to supply a private key value for import. This only works with the development version of the SmartCard-HSM.

Returns:
  the encoded C-Data for GENERATE ASYMMETRIC KEY PAIR

<static> {ByteString} SmartCardHSM.buildGAKPwithRSA(innerCAR, algo, chr, keysize, outerCAR)
Build input for Generate Asymmetric Key Pair command for generating a RSA key pair

Parameters:
{PublicKeyReference} innerCAR
  the CA the request shall be directed to
{ByteString} algo
  the public key algorithm
{PublicKeyReference} chr
  the certificate holder reference associated with this key
{Number} keysize
  the module size in bits (1024, 1536 or 2048)
{PublicKeyReference} outerCAR
  the certificate holder reference of the public key for verifying the outer signature

Returns:
  the encoded C-Data for GENERATE ASYMMETRIC KEY PAIR

<static> {ASN1} SmartCardHSM.buildKeyDomainDescription(label)
Create a PKCS#15 like KeyDomain description

Parameters:
{String} label
  the key domain label

Returns:
  the KeyDomain description

<static> {ASN1} SmartCardHSM.buildPrkDforECC(keyid, label, keysize)
Create a PKCS#15 PrivateECCKey description

Parameters:
{Number/ByteString} keyid
  the key identifier
{String} label
  the key label
keysize

Returns:
  the PrivateECCKey description

<static> {ASN1} SmartCardHSM.buildPrkDforRSA(keyid, label, modulussize)
Create a PKCS#15 PrivateRSAKey description

Parameters:
{Number/ByteString} keyid
  the key identifier
{String} label
  the key label
{Number} modulussize

Returns:
  the PrivateECCKey description

<static> {ASN1} SmartCardHSM.buildSKDforAES(keyid, label, keysize)
Create a PKCS#15 SecretKey description

Parameters:
{Number/ByteString} keyid
  the key identifier
{String} label
  the key label
{Number} keysize

Returns:
  the secret key description

changeInitializationCode(initializationCode, newInitializationCode)
Change InitializationCode

Parameters:
{ByteString} initializationCode
  current initialization code
{ByteString} newInitializationCode
  new initialization code

changeUserPIN(currentPIN, newPIN)
Change User PIN

Parameters:
{ByteString} currentPIN
  current user PIN value
{ByteString} newPIN
  new user PIN value

{Object} createXKEKKeyDomain(keyDomain, keyDomainMembership, keyDomainMembership)
Create XKEK Key Domain

Parameters:
{Number} keyDomain
  number of key domain in the range 0 to the maximum defined in the INITIALIZE DEVICE command
{ByteString} keyDomainMembership
  either a 64 byte signature (old format) or a encoded TLV object with tag 54 or 55
keyDomainMembership

Returns:
  object with properties sw{Number}, shares{Number}, outstanding{Number}, kcv{ByteString} and the key domain UID{ByteString}

decipher(keyid, algo, data)
Decipher cryptogram or agree shared secret using Diffie-Hellman

Parameters:
{Number} keyid
  the key identifier
{Number} algo
  the algorithm identifier
{ByteString} data
  the the cryptogram or concatenation of x || y of ECC public key

Returns:
  the plain output

<static> {String[]} SmartCardHSM.decodeAlgorithmList(list)
Decode algorithm list and return string array with names

Parameters:
{ByteString} list
  the algorithm list, e.g. as returned in the key meta data

Returns:
  the list of algorithm names

deleteDataObject(label)
Delete the data object references by the label.

Parameters:
{String} label
  the label of the data object

deleteFile(fid)
Delete file system object (EF or key)

Parameters:
{ByteString} fid
  the two byte file object identifier

deleteKEK(keyDomain)
Delete the key encryption key in a key domain

Parameters:
{Number} keyDomain
  the number of the key domain

deleteKeyDomain(keyDomain)
Delete the empty key domain

Parameters:
{Number} keyDomain
  the number of the key domain

{ByteString} deriveSymmetricKey(id, algo, derivationParam)
Derive Symmetric Key

Parameters:
{Number} id
  key id
{Number} algo
  algorithm id (one of ALG_CBC_ENC, ALG_CBC_DEC, ALG_CMAC or ALG_DERIVE_SP800_56C)
{ByteString} derivationParam
  the derivation parameter

Returns:
  derived key value

{Object} deriveXKEK(keyDomain, derivationParam, derivationParam)
Derive XKEK

Parameters:
{Number} keyDomain
  number of key domain in the range 0 to the maximum defined in the INITIALIZE DEVICE command
{ByteString} derivationParam
derivationParam

Returns:
  object with properties sw{Number}, shares{Number}, outstanding{Number}, kcv{ByteString} and the key domain UID{ByteString}

{Number} determineFreeCAId()
Determine an unused CA certificate identifier

Returns:
  a free CA certificate identifier or -1 if all identifier in use

<static> {ByteString} SmartCardHSM.determineFreeFid(the, the)
Determine a free FID in the list of FID for the given prefix.

Parameters:
{Number} the
  prefix to look at
{ByteString} the
  list of FID as returned from the device

Returns:
  a free two byte file identifier (FID) for the given prefix or null if range is exhausted.

<static> {Number} SmartCardHSM.determineFreeId(the, the)
Determine a free id in the list of FID for the given prefix.

Parameters:
{Number} the
  prefix to look at
{ByteString} the
  list of FID as returned from the device

Returns:
  a free id for the given prefix or -1 if range is exhausted.

{Number} determineFreeKeyId()
Determine an unused key identifier

Returns:
  a free key identifier or -1 if all key identifier in use

<static> SmartCardHSM.disableUTSRCA()
Remove Root Certificate of Development SRCA Always call this on a productive system

<static> SmartCardHSM.dumpKeyData(keydata)
Dump C-Data of Generate Asymmetric Key Pair command

Parameters:
{ByteString} keydata
  the content of C-Data

<static> {ByteString} SmartCardHSM.encodeAlgorithmList(list)
Parse and encode the algorithm list containing either algorithm ids or names

Parameters:
{String | String[]} list
  the list of algorithms

Returns:
  the algorithm list

{String[]} enumerateCACertificates()
Enumerate CA certificates

Returns:
  the list of certificate labels

{String[]} enumerateDataObjects()
Enumerate Data Objects

Returns:
  the list of data object labels

{String[]} enumerateKeys()
Enumerate key objects in the SmartCard-HSM and build the map of keys

Returns:
  the list of key labels

enumerateObjects()
Enumerate Objects

Returns:
  the enumeration

{ByteString} generateAsymmetricKeyPair(newkid, signkid, keydata)
Generate an asymmetric key pair

Parameters:
{Number} newkid
  key identifier for new key
{Number} signkid
  key identifier for signing the new public key
{ByteString} keydata
  the key data template

Returns:
  the certificate signing request containing the new public key

generateRandom(length)
Generate random data

Parameters:
{Number} length
  number of bytes

Returns:
  the random bytes

{ByteString} generateSymmetricKey(newkid, algo, keydata)
Generate a symmetric key

Parameters:
{Number} newkid
  key identifier for new key
{Number} algo
  key generation algorithm
{ByteString} keydata
  the key data template

Returns:

{ByteString} getCACertificate(label)
Return CA certificate with label

Parameters:
{String} label
  the certificate label

Returns:
  the encoded certificate

{HSMCrypto} getCrypto()
Get crypto object

Returns:
  the HSMCrypto object

{ByteString} getDataObjectFileIdentifier(label)
Return the file identifier containing the data object.

Parameters:
{String} label
  the label.

Returns:
  the two byte file identifier

{Number} getFreeMemory()
Determine free memory

Returns:
  the number of available bytes (this values is capped to 32767 on JCOP 2.4.1)

{Key} getKey(labelOrId)
Get a key reference object

Parameters:
{String/Number/ByteString} labelOrId
  label or id of key

Returns:
  the key or null if not found

getKeyDomainLabel(keyDomain)
Return the label associated with the key domain or undefined.

Parameters:
{Number} keyDomain
  the number of the key domain

{Number[]} getKeyIds()
Get key ids

Returns:
  a list of key identifier

{SmartCardHSMKey[]} getKeys()
Return a list of key objects

Returns:
  the list of keys

{String} getLabel()
Get Token Label

Returns:
  the token label from CIAInfo

{de.cardcontact.opencard.service.smartcardhsm.SmartCardHSMCardService} getNativeCardService()
Return the native OCF SmartCardHSMCardService

Returns:
  the OCF SmartCardHSMCardService

{String} getProvisioningURL()
Get ProvisioningURL

Returns:
  the configured ProvisioningURL or undefined

{ByteString} getTokenManagementKeyKCV()
Get Key Check Value of Token Management Key

Returns:
  the configured KCV of the Token Management Key or undefined

{ByteString} getTokenManagementKeySalt()
Get salt for SO-PIN derivation using the Token Management Key

Returns:
  the configured salt

{String} getVersionInfo()
Return a string describing the SmartCard-HSM Version

Returns:
  the version string

{boolean} hasDataObject(label)
Check if the data object is present

Parameters:
{String} label
  the label

Returns:
  true if the data object exists

hasFile(fid)
Try selecting the file to see if is present

Parameters:
{ByteString} fid
  the two byte file object identifier

importDataObject(label, privObj, data)
Import a data object

Parameters:
{String} label
  the unique label to reference the new data object
{Boolean} privObj
  true to store the data object with read protection
{ByteString} data
  the data blob to store

importEncryptedKeyShare(keyshare, password, keyDomain)
Decrypt and import a DKEK share

Parameters:
{ByteString} keyshare
  the encrypted key share as read from the .pbe file
{ByteString} password
  the password
{Number} keyDomain
  the number of the key domain

Returns:
  object with properties sw{Number}, shares{Number}, outstanding{Number} and kcv{ByteString}

{Object} importKeyShare(keyDomain, keyshare)
Import DKEK share or query status

Parameters:
{Number} keyDomain
  the number of the key domain
{ByteString} keyshare
  32 byte key share

Returns:
  object with properties sw{Number}, shares{Number}, outstanding{Number} and kcv{ByteString}

initDevice(options, initialPIN, initializationCode, retryCounterInitial, keyshares)
Initialize device and clear all keys and files

Parameters:
{ByteString} options
  two byte option mask
{ByteString} initialPIN
  initial user PIN value
{ByteString} initializationCode
  secret code for device initialization (set during first use)
{Number} retryCounterInitial
  retry counter for user PIN
{Number} keyshares
  number of device key encryption key shares (optional)

{Boolean} isInitialized()
Return true is SmartCard-HSM is initialized

Returns:
  true if initialized

{Boolean} isPINResetEnabled()
Check if the RESET RETRY COUNTER command can reset the PIN

Returns:
  true if enable during initialization

{Boolean} isResetRetryCounterEnabled()
Check if the RESET RETRY COUNTER command is enabled

Returns:
  true if enable during initialization

logout()
Logout

{ISOSecureChannel} openSecureChannel(crypto, devAuthPK)
Open a secure channel using device authentication

Parameters:
{Crypto} crypto
  the crypto provider to use
{Key} devAuthPK
  the device authentication public key
{Number} Key.AES
  or Key.DES to request AES or DES secure messaging (Default probe)

Returns:
  the initialized secure channel

<static> {CVC[]} SmartCardHSM.parseCertificateList(a)
Parse list of CVC in a binary blob

Parameters:
{ByteString} a
  binary blob (e.g an EF) containing concatenated CVCs

Returns:
  the list of CVCs

{object} parseKeyDomainStatus(status)
Parse the key domain status returned from the device

Parameters:
{ByteString} status
  the R-DATA from the MANAGE KEY DOMAIN command

Returns:
  the decoded status Info

{Number} queryInitializationCodeStatus()
Request Initialization Code Status

Returns:
  the status word SW1/SW2 returned by the device

{Object} queryKeyDomainStatus(keyDomain)
Query the status of the key domain

Parameters:
{Number} keyDomain
  the number of the key domain which will be queried, default is 0

Returns:
  object with properties sw{Number}, shares{Number}, outstanding{Number}, kcv{ByteString} and for a XKEK key domain the key domain UID{ByteString}

{Number} queryPINStatus(p2)
Request PIN Status Information

Parameters:
{Number} p2
  the PIN object id

Returns:
  the status word SW1/SW2 returned by the device

{Number} queryUserPINStatus()
Request PIN Status Information

Returns:
  the status word SW1/SW2 returned by the device

{ByteString} readBinary(fid, offset, length)
Read transparent EF referenced by file identifier

Parameters:
{ByteString} fid
  the two byte file identifier (optional - use currently selected EF if absent)
{Number} offset
  the offset into the EF (optional)
{Number} length
  the number of byte to read (optional)

Returns:
  the data read from the EF

selectFile(fid)
Select the file or key an return the FCP

Parameters:
{ByteString} fid
  the two byte file object identifier

<static> SmartCardHSM.setTrustedSRCACertificates(srcalist)
Set the list of trusted SRCA certificates

Parameters:
{ByteString[]} srcalist
  the list of binary encoded SRCA certificates

sign(keyid, algo, data)
Sign data using referenced key

Parameters:
{Number} keyid
  the key identifier for signing
{algo} algo
  the algorithm identifier
{ByteString} data
  the data to be signed

Returns:
  the signature value

<static> {ByteString} SmartCardHSM.stripLeadingZeros(value)
Strips leading zeros of a ByteString

Parameters:
{ByteString} value
  the ByteString value

Returns:
  the stripped ByteString object, may be an empty ByteString

unblockUserPIN(initializationCode, newPIN)
Unblock and set User PIN

Parameters:
{ByteString} initializationCode
  the initialization code
{ByteString} newPIN
  new user PIN value (optional)

unwrapAndReplaceKey(id, keyblob)
Replace symmetric key value encrypted under current key

Parameters:
{Number} id
  key id
{ByteString} keyblob
  the wrapped key

unwrapKey(id, keyblob)
Unwrap key with DKEK

Parameters:
{Number} id
  key id
{ByteString} keyblob
  the wrapped key

updateBinary(fid, offset, data)
Update transparent EF referenced by file identifier

Parameters:
{ByteString} fid
  the two byte file identifier
{Number} offset
  the offset into the EF
{ByteString} data
  the data to write

updateKey(key)
Update key attributes, in particular the use counter

Parameters:
{HSMKey} key
  the HSM key

{Key} validateCertificateChain(crypto)
Validate device certificate chain

Parameters:
{Crypto} crypto
  the crypto provider to use

Returns:
  the device authentication public key

<static> {Key} SmartCardHSM.validateCertificateChain(crypto, devAutCert)
Validate device certificate chain

Parameters:
{Crypto} crypto
  the crypto provider to use
{ByteString} devAutCert
  the device certificate chain read from EF.C_DevAut

Returns:
  the device authentication public key

verifyCertificate(cvc)
Verify card verifiable certificate

Parameters:
{CVC} cvc
  the card verifiable certificate

verifyUserPIN(userPIN)
Verify User PIN

Parameters:
{ByteString} userPIN
  user PIN value

Returns:
  the status word SW1/SW2 returned by the device

{ByteString} wrapKey(id)
Wrap key under DKEK

Parameters:
{Number} id
  key id

Returns:
  key blob with encrypted key value

Documentation generated by JsDoc Toolkit 2.4.0 on Mon Feb 23 2026 11:18:10 GMT+0100 (CET)