Class Index | File Index

## Classes

- _global_
- AccessController
- APDU
- AuthenticationObject
- CAConnection
- ChipAuthentication
- ChipAuthenticationDomainParameterInfo
- ChipAuthenticationInfo
- ChipAuthenticationPublicKeyInfo
- CommandInterpreter
- CRLGenerator
- CVC
- CVCCA
- CVCertificateStore
- DataUnitAPDU
- DF
- DKEK
- DNEncoder
- EAC20
- EAC2CVCertificateGenerator
- EAC2CVRequestGenerator
- FCP
- File
- FileEncryptor
- FileSelector
- FileSystemIdObject
- FSNode
- GPSCP03
- HSMCVCertificateStore
- HSMKeyStore
- LinearEF
- ManagePKA
- P11CVCertificateStore
- PACE
- PACEDomainParameterInfo
- PACEInfo
- PaperKeyEncoding
- PKCS10Generator
- PublicKeyFile
- PublicKeyReference
- RAMClient
- RestrictedIdentificationDomainParameterInfo
- RestrictedIdentificationInfo
- SecureChannelHandler
- SecureMessagingCommandAPDUDecoder
- SecurityEnvironment
- SignatureKey
- SmartCardHSM
- SmartCardHSMCrypto
- SmartCardHSMInitializer
- SmartCardHSMKey
- SmartCardHSMKeySpecGenerator
- SmartCardHSMSymmetricKeySpecGenerator
- TransparentEF
- TrustAnchor
- X509CertificateGenerator
- X509CertificateIssuer
- X509CertificateStore
- X509Signer

# Class SmartCardHSMInitializer

Class implementing the device initialization methods
Defined in: SmartCardHSM.js.

Class Summary
Constructor Attributes | Constructor Name and Description
--- | ---
| SmartCardHSMInitializer(card) Initialize SmartCard-HSM

Method Summary
Method Attributes | Method Name and Description
--- | ---
| initialize() Perform Initialization
| setBioTemplate(slot, aid, param) Select the biometric matching server for a one of the biometric templates
| setCombinedAuthenticationMode(enable) Enable the combined authentication mode of user pin and public key authentication.
| setDKEKShares(keyshares) Set the number of DKEK shares
| setInitializationCode(initializationCode) Set the initialization code
| setKeyDomains(keyDomains) Set the number of key domains
| setLabel(label) Set the label to be written to a minimal CIAInfo in EF 2F03
| setProvisioningURL(provisioningURL) Set the provisioning URL to be written to fixed parameter in CB00.
| setPublicKeyAuthenticationParameter(requiredPublicKeysForAuthentication, numberOfPublicKeys) Set parameter for public key authentication with n-of-m scheme, namely the values for n and m
| setReplacePKAKeyMode(enable) Enable or disable replacing of a PKA key
| setResetRetryCounterMode(enable) Enable or disable RESET RETRY COUNTER command
| setResetRetryCounterResetOnlyMode(resetOnly) If enabled RESET RETRY COUNTER only resets the error counter.
| setRetryCounterInitial(retryCounterInitial) Set the retry counter The SmartCard-HSM enforces a retry counter <= 3 for PIN length 6 The SmartCard-HSM enforces a retry counter <= 5 for PIN length 7 The SmartCard-HSM enforces a retry counter <= 10 for PIN length larger than 7
| setSessionPINMode(0) Enable or disable session PIN mode
| setTokenManagementKey(kcv, salt) Set the key check value of the token management key and the optional salt used for SO-PIN derivation
| setTransportPINMode(enable) Enable or disable transport PIN mode
| setUserPIN(userPIN) Set the User PIN

Class Detail
SmartCardHSMInitializer(card)
Initialize SmartCard-HSM

Parameters:
{Card} card
  the card object

Method Detail
initialize()
Perform Initialization

setBioTemplate(slot, aid, param)
Select the biometric matching server for a one of the biometric templates

Parameters:
{Number} slot
  either 0 or 1 for first or second template
{ByteString} aid
  the application identifier of the on-card biometric server
{Number} param
  one byte parameter passed to the server during initialization

setCombinedAuthenticationMode(enable)
Enable the combined authentication mode of user pin and public key authentication.

Parameters:
{Boolean} enable
  true (non-default) to require public key authentication and user authentication

setDKEKShares(keyshares)
Set the number of DKEK shares

Parameters:
{Number} keyshares
  number of DKEK shares in the range 0 to 255

setInitializationCode(initializationCode)
Set the initialization code

Parameters:
{ByteString} initializationCode
  an 8 byte code

setKeyDomains(keyDomains)
Set the number of key domains

Parameters:
{Number} keyDomains
  number of key domains

setLabel(label)
Set the label to be written to a minimal CIAInfo in EF 2F03

Parameters:
{String} label
  the label

setProvisioningURL(provisioningURL)
Set the provisioning URL to be written to fixed parameter in CB00.

Parameters:
{String} provisioningURL
  the URL at which this SE will be provisioned

setPublicKeyAuthenticationParameter(requiredPublicKeysForAuthentication, numberOfPublicKeys)
Set parameter for public key authentication with n-of-m scheme, namely the values for n and m

Parameters:
{Number} requiredPublicKeysForAuthentication
  number of key that must be authenticated for access
{Number} numberOfPublicKeys
  to register

setReplacePKAKeyMode(enable)
Enable or disable replacing of a PKA key

Parameters:
{Boolean} enable
  true (non-default) to allow replacing of a PKA key

setResetRetryCounterMode(enable)
Enable or disable RESET RETRY COUNTER command

Parameters:
{Boolean} enable
  true (default) to allow RESET RETRY COUNTER command to reset user PIN using the initialization code

setResetRetryCounterResetOnlyMode(resetOnly)
If enabled RESET RETRY COUNTER only resets the error counter. Otherwise RRC allows changing the PIN

Parameters:
{Boolean} resetOnly
  true to only reset the error counter, false otherwise (default)

setRetryCounterInitial(retryCounterInitial)
Set the retry counter The SmartCard-HSM enforces a retry counter <= 3 for PIN length 6 The SmartCard-HSM enforces a retry counter <= 5 for PIN length 7 The SmartCard-HSM enforces a retry counter <= 10 for PIN length larger than 7

Parameters:
{Number} retryCounterInitial
  in the range 1 to 10.

setSessionPINMode(0)
Enable or disable session PIN mode

Parameters:
{Number} 0
  - disable, 1 - enable with clear-on-reset 3 - enable with explicit clearing

setTokenManagementKey(kcv, salt)
Set the key check value of the token management key and the optional salt used for SO-PIN derivation

Parameters:
{ByteString} kcv
  the key check value of the token management key
{ByteString} salt
  the salt used to derive the SO-PIN

setTransportPINMode(enable)
Enable or disable transport PIN mode

Parameters:
{Boolean} enable
  true (non-default) to set user PIN to transport state

setUserPIN(userPIN)
Set the User PIN

Parameters:
{ByteString} userPIN
  a 6 to 16 byte code

Documentation generated by JsDoc Toolkit 2.4.0 on Thu Apr 30 2026 15:08:16 GMT+0200 (CEST)