Class Index | File Index

## Classes

- _global_
- AccessController
- APDU
- AuthenticationObject
- CAConnection
- ChipAuthentication
- ChipAuthenticationDomainParameterInfo
- ChipAuthenticationInfo
- ChipAuthenticationPublicKeyInfo
- CommandInterpreter
- CRLGenerator
- CVC
- CVCCA
- CVCertificateStore
- DataUnitAPDU
- DF
- DKEK
- DNEncoder
- EAC20
- EAC2CVCertificateGenerator
- EAC2CVRequestGenerator
- FCP
- File
- FileEncryptor
- FileSelector
- FileSystemIdObject
- FSNode
- GPSCP03
- HSMCVCertificateStore
- HSMKeyStore
- LinearEF
- ManagePKA
- P11CVCertificateStore
- PACE
- PACEDomainParameterInfo
- PACEInfo
- PaperKeyEncoding
- PKCS10Generator
- PublicKeyFile
- PublicKeyReference
- RAMClient
- RestrictedIdentificationDomainParameterInfo
- RestrictedIdentificationInfo
- SecureChannelHandler
- SecureMessagingCommandAPDUDecoder
- SecurityEnvironment
- SignatureKey
- SmartCardHSM
- SmartCardHSMCrypto
- SmartCardHSMInitializer
- SmartCardHSMKey
- SmartCardHSMKeySpecGenerator
- SmartCardHSMSymmetricKeySpecGenerator
- TransparentEF
- TrustAnchor
- X509CertificateGenerator
- X509CertificateIssuer
- X509CertificateStore
- X509Signer

# Class ManagePKA

Class providing support for public key authentication
Defined in: ManagePKA.js.

Class Summary
Constructor Attributes | Constructor Name and Description
--- | ---
| ManagePKA(sc, deviceId) Manage Public Key Authentication

Method Summary
Method Attributes | Method Name and Description
--- | ---
| canEnumeratePublicKeys() Check if registered public keys can be enumerated
| checkKeyStatus(chr) Check status of public key
| describeStatus() Describe current status in human readable form
| enumeratePublicKeys() Enumerate names (CHR) or registered public keys
| getAuthenticatedPublicKeys() Get number of keys already authenticated in this session
| getMissingPublicKeys() Get number of public keys missing for complete setup
| getNumberOfPublicKeys() Get number of public keys (m)
| getRequiredPublicKeysForAuthentication() Get number of keys required for successfull authentication (n)
| isActive() Check if public key authentication is active for device
| performAuthentication(srcsc, key) Perform authentication with source SmartCard-HSM and key on that device
| registerPublicKey(pk, devcert, dicacert, replace) Validate and register public key

Class Detail
ManagePKA(sc, deviceId)
Manage Public Key Authentication

Parameters:
{SmartCardHSM} sc
  the SmartCard-HSM used as target for PKA
{ByteString} deviceId
  the device id as returned by getCHR().getBytes() for the device certificate

Method Detail
{boolean} canEnumeratePublicKeys()
Check if registered public keys can be enumerated

Returns:
  true if enumeration is supported

{Number} checkKeyStatus(chr)
Check status of public key

Parameters:
{PublicKeyReference} chr
  the public key reference under which the public key is registered

Returns:
  ManagePKA.KEY_PRESENT if key is registered in SmartCard-HSM, ManagePKA.KEY_NOT_FOUND if not. ManagePKA.KEY_ALREADY_AUTHENTICATED is returned if the public key has already been authenticated

{String} describeStatus()
Describe current status in human readable form

Returns:
  the status

{Object} enumeratePublicKeys()
Enumerate names (CHR) or registered public keys

Returns:
  Object with property chr containing the PublicKeyReference and with property status containing ManagePKA.KEY_PRESENT if a key is registered at that slot, ManagePKA.KEY_NOT_FOUND if not. ManagePKA.KEY_ALREADY_AUTHENTICATED is returned if the public key has already been authenticated.

{Number} getAuthenticatedPublicKeys()
Get number of keys already authenticated in this session

Returns:
  the number of keys already authenticated in this session

{Number} getMissingPublicKeys()
Get number of public keys missing for complete setup

Returns:
  the number of public keys missing for complete setup

{Number} getNumberOfPublicKeys()
Get number of public keys (m)

Returns:
  the number of public keys (m)

{Number} getRequiredPublicKeysForAuthentication()
Get number of keys required for successfull authentication (n)

Returns:
  the number of keys required for successfull authentication (n)

{boolean} isActive()
Check if public key authentication is active for device

Returns:
  true if supported and active

performAuthentication(srcsc, key)
Perform authentication with source SmartCard-HSM and key on that device

Parameters:
{SmartCardHSM} srcsc
  the SmartCard-HSM containing the private key for authentication
{Key} key
  the private key

registerPublicKey(pk, devcert, dicacert, replace)
Validate and register public key

Parameters:
{CVC} pk
  public key in CSR format from card
{CVC} devcert
  device certificate
{CVC} dicacert
  device issuer certificate
{Number} replace
  the id of the key to be replaced (0-based) or undefined

Documentation generated by JsDoc Toolkit 2.4.0 on Thu Apr 30 2026 15:08:16 GMT+0200 (CEST)